**ARTICLE 14 – FLOODPLAIN MANAGEMENT**

**14.1 Purpose and Establishment**

Certain areas of the Town of Buxton, Maine are subject to periodic flooding, causing serious damages to properties within these areas. Relief is available in the form of flood insurance as authorized by the National Flood Insurance Act of 1968.

Therefore, the Town of Buxton, Maine has chosen to become a participating community in the National Flood Insurance Program, and agrees to comply with the requirements of the National Flood Insurance Act of 1968 (P.L. 90-488, as amended) as delineated in this Floodplain Management Ordinance.

It is the intent of the Town of Buxton, Maine to require the recognition and evaluation of flood hazards in all official actions relating to land use in the floodplain areas having special flood hazards.

The Town of Buxton has the legal authority to adopt land use and control measures to reduce future flood losses pursuant to Title 30-A MRSA, Sections 3001-3007, 4352 and 4401-4407.

The National Flood Insurance Program, established in the aforesaid Act, provides that areas of the Town of Buxton having a special flood hazard be identified by the Federal Emergency Management Agency and that floodplain management measures be applied in such flood hazard areas. This Ordinance establishes a Flood Hazard Development Permit system and review procedure for development activities in the designated flood hazard areas of the Town of Buxton, Maine.

The areas of special flood hazard, Zones A and A1-3O, are identified by the Federal Emergency Management Agency in a report entitled "Flood Insurance Study - Town of Buxton, Maine, York County," dated January 5, 1982 with accompanying "Flood Insurance Rate Map" dated July 5, 1982 and "Flood Boundary and Floodway Map" dated July 5, 1982 which are hereby adopted by reference and declared to be a part of this Ordinance.

**14.2 Permit Required**

Before any construction or other development (as defined in Article 2), including the placement of manufactured homes, begins within any areas of special flood hazard established in Section 14.1, a Flood Hazard Development Permit shall be obtained from the Code Enforcement Officer. This permit shall be in addition to any other permits which may be required pursuant to the codes and ordinances of the Town of Buxton, Maine.

**14.3 Application for Permit**

The application for a Flood Hazard Development Permit shall be submitted to the Code Enforcement Officer and shall include:

1. The name, address and phone number of the applicant, owner, and contractor;
2. An address and a map indicating the location of the construction site;
3. A site plan showing location of existing and/or proposed development, including but not limited to structures, sewage disposal facilities, water supply facilities, areas to be cut and filled, and lot dimensions;
4. A statement of the intended use of the structure and/or development;
5. A statement of the cost of the development including all materials and labor;
6. A statement as to the type of sewage system proposed;
7. Specification of dimensions of the proposed structure and/or development;

[Items H-K.2 apply only to new construction and substantial improvements.]

1. The elevation in relation to the National Geodetic Vertical Datum (NGVD), or to a locally established datum in Zone A only, of the:

14.3.H.1. base flood at the proposed site of all new or substantially improved structures, which is determined:

(a.) in Zones A1-30, from data contained in the "Flood Insurance Study - Town of Buxton, Maine," as described in Section 14.1; or,

(.b.) in Zone A, to be the elevation of the ground at the intersection of the floodplain boundary and a line perpendicular to the shoreline which passes along the ground through the site of the proposed building;

14.3.H.2. highest and lowest grades at the site adjacent to the walls of the proposed building;

14.3.H.3. lowest floor, including basement; and whether or not such structures contain a basement; and,

14.3.H.4. level, in the case of non-residential structures only, to which the structure will be floodproofed;

1. A description of an elevation reference point established on the site of all new or substantially improved structures;
2. Either an Elevation Certificate (FEMA Form 81-31, 03/97, as amended) completed by a Professional Land Surveyor, registered professional engineer or architect; or, for non-residential structures to be floodproofed, a Floodproofing Certificate (FEMA Form 81-65, 05/93, as amended) completed by a registered professional engineer or architect. These Certificates verify that the elevations shown on the application are accurate.

14.3.J Certifications as required in Section 14.6 by a registered professional engineer or architect that:

14.3.K A description of the extent to which any water course will be altered or relocated as a result of the proposed development; and,

14.3.K.1. floodproofing methods for any non-residential structures will meet the floodproofing criteria of Subsection 14.3.H.4.; Section 14.6.G.; and other applicable standards in Section 14.6;

14.3.K.2. engineered hydraulic openings in foundation walls will meet the standards of Subsection 14.6.L.2.;

14.3.K.3. bridges will meet the standards of Section 14.6.M.,

14.3.K.4. containment walls will meet the standards of Section 14.6.N.,

14.3.L A statement of construction plans describing in detail how each applicable development standard in Section 14.6 will be met.

**14.4 Application Fee and Expert's Fee**

A non-refundable application fee of $25.00 shall be paid to the Town Clerk and a copy of a receipt for the same shall accompany the application.

An additional fee may be charged if the Code Enforcement Officer and/or Board of Appeals need the assistance of a professional engineer or other expert. The expert's fee shall be paid in full by the applicant within 10 days after the town submits a bill to the applicant. Failure to pay the bill shall constitute a violation of the ordinance and be grounds for the issuance of a stop work order. An expert shall not be hired by the municipality at the expense of an applicant until the applicant has either consented to such hiring in writing or been given an opportunity to be heard on the subject. An applicant who is dissatisfied with a decision of the Code Enforcement Officer may appeal that decision to the Board of Appeals.

**14.5 Review Standards For Flood Hazard Development Permit Applications**

The Code Enforcement Officer shall:

14.5.A Review all applications for the Flood Hazard Development Permit to assure that proposed developments are reasonably safe from flooding and to determine that all pertinent requirements of Section 14.6 (Development Standards) have, or will be met;

14.5.B Utilize, in the review of all Flood Hazard Development Permit applications, the base flood data contained in the "Flood Insurance Study - Town of Buxton, Maine," as described in Section 14.1. In special flood hazard areas where base flood elevation data are not provided, the Code Enforcement Officer shall obtain, review and reasonably utilize any base flood elevation and floodway data from federal, state, or other sources, including information obtained pursuant to Subsection 14.3.H.1.b.; Section 14.6.K.; and Section 14.8.D., in order to administer Section 14.6 of this Ordinance;

14.5.C Make interpretations of the location of boundaries of special flood hazard areas shown on the maps described in Section 14.1 of this Ordinance;

14.5.D In the review of Flood Hazard Development Permit applications, determine that all necessary permits have been obtained from those federal, state, and local government agencies from which prior approval is required by federal or state law, including but not limited to Section 404 of the Federal Water Pollution Control Act Amendments of 1972, 33 U.S.C. 1334;

14.5.E Notify adjacent municipalities, the Department of Environmental Protection, and the Maine Floodplain Management Program in the State Planning Office prior to any alteration or relocation of a water course and submit copies of such notifications to the Federal Emergency Management Agency;

14.5.F Issue one of the following Flood Hazard Development Permits based on the type of development:

14.5.F.1 Issue a two-part Flood Hazard Development Permit for elevated

structures. Part I shall authorize the applicant to build a structure to and including

the first horizontal floor only above the base flood level. At that time the applicant shall provide the Code Enforcement Officer with a second Elevation Certificate completed by a Professional Land Surveyor, registered professional engineer or architect based on the Part I permit construction, “as built”, for verifying compliance with the elevation requirements of Section 14.6, paragraphs F, G, or H. Following review of the Elevation Certificate data, which shall take place within 72 hours of receipt of the application, the Code Enforcement Officer shall issue Part II of the Flood Hazard Development Permit. Part II shall authorize the applicant to complete the construction project; or,

14.5.F.2. Issue a Flood Hazard Development Permit for Floodproofing of Non-Residential Structures that are new construction or substantially improved non-residential structures that are not being elevated but that meet the floodproofing standards of Subsection 14.6.G.1.a.,b., and c. The application for this permit shall include a Floodproofing Certificate signed by a registered professional engineer or architect; or,

14.5.F.3. Issue a Flood Hazard Development Permit for Minor Development for all development that is not new construction or a substantial improvement, such as repairs, maintenance, renovations, or additions, whose value is less than 50% of the market value of the structure. Minor development also includes, but is not limited to: accessory structures as provided for in Section 14.6.J., mining, dredging, filling, grading, paving, excavation, drilling operations, storage of equipment or materials, deposition or extraction of materials, public or private sewage disposal systems or water supply facilities that do not involve structures; and non-structural projects such as bridges, dams, towers, fencing, pipelines, wharves and piers.

14.5.G Maintain, as a permanent record, copies of all Flood Hazard Development Permit Applications, corresponding Permits issued, and data relevant thereto, including reports of the Board of Appeals on variances granted under the provisions of Section 14.9 of this Ordinance, and copies of Elevation Certificates, Floodproofing Certificates, Certificates of Compliance and certifications of design standards required under the provisions of Sections 14.3, 14.6, and 14.7 of this Ordinance.

**14.6 Development Standards**

All developments in areas of special flood hazard shall meet the following applicable standards:

1. All Development **-** All development shall:

14.6.A.1. be designed or modified and adequately anchored to prevent flotation

(excluding piers and docks), collapse or lateral movement of the development resulting from hydrodynamic and hydrostatic loads, including the effects of buoyancy;

14.6.A.2. use construction materials that are resistant to flood damage;

14.6.A.3. use construction methods and practices that will minimize flood damage; and,

14.6.A.4. use electrical, heating, ventilation, plumbing, and air conditioning equipment, and other service facilities that are designed and/or located so as to prevent water from entering or accumulating within the components during flooding conditions.

1. Water Supply **-** All new and replacement water supply systems shall be designed to minimize or eliminate infiltration of flood waters into the systems.
2. Sanitary Sewage Systems **-** All new and replacement sanitary sewage systems shall be designed and located to minimize or eliminate infiltration of flood waters into the system and discharges from the system into flood waters.
3. On Site Waste Disposal Systems -On site waste disposal systems shall be located and constructed to avoid impairment to them or contamination from them during floods.
4. Watercourse Carrying Capacity - All development associated with altered or relocated portions of a watercourse shall be constructed and maintained in such a manner that no reduction occurs in the flood carrying capacity of the watercourse.

14.6.F Residential - No new construction permitted. Reconstruction, Replacement or substantial improvement of any existing residential structure located within:

14.6.F.1. Zones A1-30 shall have the lowest floor (including basement) elevated to at least one foot above the base flood elevation.

14.6.F.2. Zone A shall have the lowest floor (including basement) elevated to at least one foot above the base flood elevation utilizing information obtained pursuant to Subsection14.3.H.1.b.; Section 14.5.B; or Section 14.8.D.

14.6.GNon Residential - New construction or substantial improvement of any non-residential structure located within:

14.6.G.1. Zones A1-30 shall have the lowest floor (including basement) elevated to at least one foot above the base flood elevation, or together with attendant utility and sanitary facilities shall:

(a.) be floodproofed to at least one foot above the base flood elevation so that below that elevation the structure is watertight with walls substantially impermeable to the passage of water;

1. have structural components capable of resisting hydrostatic and hydrodynamic loads and the effects of buoyancy; and,

(c.) be certified by a registered professional engineer or architect that the floodproofing design and methods of construction are in accordance with accepted standards of practice for meeting the provisions of this section. Such certification shall be provided with the application for a Flood Hazard Development Permit, as required by Section 14.3.K. and shall include a record of the elevation above mean sea level to which the structure is floodproofed.

14.6.G.2. Zone A shall have the lowest floor (including basement) elevated to at least one foot above the base flood elevation utilizing information obtained pursuant to Subsection 14.3.H.1.b.; Section 14.5.B; or Section 14.8.D., or

(a.) together with attendant utility and sanitary facilities meet the floodproofing standards of Subsection 14.6.G.1.

14.6.HManufactured Homes - No new manufactured homes permitted. Reconstruction, Replacement, or **s**ubstantial improvement of any existing manufactured homes located within:

14.6.H.1. Zones A1-30 shall:

(.a.) be elevated such that the lowest floor (including basement) of the manufactured home is at least one foot above the base flood elevation.

(b.) be on a permanent foundation, which may be poured masonry slab or foundation walls, with hydraulic openings, or may be reinforced piers or block supports, any of which support the manufactured home so that no weight is supported by its wheels and axles; and,

(c.) be securely anchored to an adequately anchored foundation system to resist flotation, collapse, or lateral movement. Methods of anchoring may include but are not limited to:

(i.) over-the-top ties anchored to the ground at the four corners of the manufactured home, plus two additional ties per side at intermediate points (manufactured homes less than 50 feet long require one additional tie per side); or by,

(ii.) frame ties at each corner of the home, plus five additional ties along each side at intermediate points (manufactured homes less than 50 feet long require four additional ties per side).

(iii.) all components of the anchoring system described in Section 14.6, paragraph H.1.c.i. & ii shall be capable of carrying a force of 4800 pounds.

14.6.H.2. Zone A shall:

(a.) be elevated on a permanent foundation, as described in Section 14.6.H.1.b., such that the lowest floor (including basement) of the manufactured home is at least one foot above the base flood elevation utilizing information obtained pursuant to Subsection 14.3.H.1.b.; Section 14.5.B; or Section 14.8.D.; and

(b.) meet the anchoring requirements of Subsection 14.6.H.1.c.

14.6.IRecreational Vehicles - Recreational Vehicles located within:

14.6.I.1 Zones A1-30 shall either:

14.6.I.1.a. be on the site for fewer than 180 consecutive days,

14.6.I.1.b. be fully licensed and ready for highway use. A recreational vehicle is ready for highway use if it is on its wheels or jacking system, is attached to the site only by quick disconnect type utilities and security devices, and has no permanently attached additions; or,

14.6.I.1.c. be permitted in accordance with the elevation and anchoring requirements for "manufactured homes" in Section 14.6.H.1.

14.6.J **Accessory** Structures - Accessory Structures, as defined in Article 2, located within Zones A1-30 and A, shall be exempt from the elevation criteria required in Section 14.6.F. & G. above, if all other requirements of Section 14.6 and all the following requirements are met. Accessory Structures shall:

14.6.J.1. be 500 square feet or less and have a value less than $3000;

14.6.J.2. have unfinished interiors and not be used for human habitation;

14.6.J.3. have hydraulic openings, as specified in Subsection 14.6.L.2., in

at least two different walls of the accessory structure;

14.6.J.4. be located outside the floodway;

14.6.J.5. when possible be constructed and placed on the building site so as to offer the minimum resistance to the flow of floodwaters and be placed further from the source of flooding than is the primary structure; and,

14.6.J.6. have only ground fault interrupt electrical outlets. The electric service disconnect shall be located above the base flood elevation and when possible outside the Special Flood Hazard Area.

14.6.K Floodways

14.6.K.1. In Zones A1-30, encroachments, including fill, new construction, substantial improvement, and other development shall not be permitted in riverine areas, for which a regulatory floodway is designated on the community's Flood Boundary and Floodway Map, unless a technical evaluation certified by a registered professional engineer is provided demonstrating that such encroachments will not result in any increase in flood levels within the community during the occurrence of the base flood discharge.

14.6.K.2. In Zones A1-30 and A riverine areas for which no regulatory floodway is designated, encroachments, including fill, new construction, substantial improvement, and other development shall not be permitted in the floodway as determined in Subsection 14.6.K.3. unless a technical evaluation certified by a registered professional engineer is provided demonstrating that the cumulative effect of the proposed development, when combined with all other existing development and anticipated development:

14.6.K.2.a. will not increase the water surface elevation of the base flood more than one foot at any point within the community; and,

14.6.K.2.b. is consistent with the technical criteria contained in Chapter 5 entitled "Hydraulic Analyses," *Flood Insurance Study - Guidelines and Specifications for Study Contractors*, (FEMA 37/ January 1995, as amended).

14.6.K.3. In Zones A1-30 and A riverine areas for which no regulatory floodway is designated, the regulatory floodway is determined to be the channel of the river or other water course and the adjacent land areas to a distance of one-half the width of the floodplain as measured from the normal high-water mark to the upland limit of the floodplain.

14.6.LEnclosed Areas Below the Lowest Floor **-** New construction or substantial improvement of any structure in Zones A1-30 and A that meets the development standards of Section 14.6, including the elevation requirements of Section 14.6, paragraphs F, G, or H and is elevated on posts, columns, piers, piles, "stilts," or crawlspaces may be enclosed below the base flood elevation requirements provided all the following criteria are met or exceeded:

14.6.L.1. Enclosed areas are not "basements" as defined in Section 14.8;

14.6.L.2. Enclosed areas shall be designed to automatically equalize hydrostatic flood forces on exterior walls by allowing for the entry and exit of flood water. Designs for meeting this requirement must either:

14.6.L.2.a. be engineered and certified by a registered professional engineer or architect; or,

14.6.L.2.b. meet or exceed the following minimum criteria:

14.6.L.2.b.i. a minimum of two openings having a total net area of not less than one square inch for every square foot of the enclosed area;

14.6.L.2.b.ii. the bottom of all openings shall be no higher than one foot above the lowest grade; and,

14.6.L.2.b.iii. openings may be equipped with screens, louvers, valves, or other coverings or devices provided that they permit the entry and exit of flood waters automatically without any external influence or control such as human intervention, including the use of electrical and other non-automatic mechanical means;

14.6.L.3. The enclosed area shall not be used for human habitation; and,

14.6.L.4. The enclosed areas are usable solely for building access, parking of vehicles, or storing of articles and equipment used for maintenance of the building.

14.6**.**M Bridges - New construction or substantial improvement of any bridge in Zones A1-30 and A shall be designed such that:

14.6.M.1. when possible, the lowest horizontal member (excluding the pilings, or columns) is elevated to at least one foot above the base flood elevation; and

14.6.M.2. a registered professional engineer shall certify that:

14.6.M.2.a. the structural design and methods of construction shall meet the elevation requirements of this section and the floodway standards of Section 14.6.K.; and

14.6.M.2.b. The foundation and superstructure attached thereto is anchored to resist flotation, collapse, and lateral movement due to the effects of wind and water loads acting simultaneously on all structural components. Water loading values used shall be those associated with the base flood.

14.6.NContainment Walls **-** New construction or substantial improvement of any containment wall located within:

14.6.N.1. Zones A1-30 and A shall:

14.6.N.1.a. have the containment wall elevated to at least one foot above the base flood elevation;

14.6.N.1.b. have structural components capable of resisting hydrostatic and hydrodynamic loads and the effects of buoyancy; and,

14.6.N.1.c. be certified by a registered professional engineer or architect that the design and methods of construction are in accordance with accepted standards of practice for meeting the provisions of this section. Such certification shall be provided with the application for a Flood Hazard Development Permit, as required by Section 14.3.K.

14.6.OWharves, Piers and Docks- New construction or substantial improvement of wharves, piers, and docks are permitted in Zones A1-30, and A, in and over water and seaward of the mean high tide if the following requirements are met:

14.6.O.1. wharves, piers, and docks shall comply with all applicable local, state, and federal regulations; and

14.6.O.2. for commercial wharves, piers, and docks, a registered professional engineer shall develop or review the structural design, specifications, and plans for the construction.

**14.7 Certificate Of Compliance**

No land in a special flood hazard area shall be occupied or used and no structure, which is constructed or substantially improved shall be occupied until a Certificate of Compliance is issued by the Code Enforcement Officer subject to the following provisions:

1. For New Construction or Substantial Improvement of any structure the applicant shall submit to the Code Enforcement Officer, an Elevation Certificate completed by a Professional Land Surveyor, registered professional engineer, or architect, for compliance with Section 14.6, paragraphs F, G, or H.

1. The applicant shall submit written notification to the Code Enforcement Officer that the development is complete and complies with the provisions of this ordinance.

1. Within 10 working days, the Code Enforcement Officer shall:

14.7.C.1. review the Elevation Certificate and the applicant’s written notification; and,

14.7.C.2. upon determination that the development conforms with the provisions of this ordinance, shall issue a Certificate of Compliance.

**14.8 Review Of Subdivision And Development Proposals**

The Planning Board shall, when reviewing subdivisions and other proposed developments that require review under other federal law, state law or local ordinances or regulations and all projects on 5 or more acres, or in the case of manufactured home parks divided into two or more lots, assure that:

1. All such proposals are consistent with the need to minimize flood damage.
2. All public utilities and facilities, such as sewer, gas, electrical and water systems are located and constructed to minimize or eliminate flood damages.
3. Adequate drainage is provided so as to reduce exposure to flood hazards.
4. All proposals include base flood elevations, flood boundaries, and, in a riverine floodplain, floodway data. These determinations shall be based on engineering practices recognized by the Federal Emergency Management Agency.

14.8.E Any proposed development plan must include a condition of plan approval requiring that structures on any lot in the development having any portion of its land within a Special Flood Hazard Area, are to be constructed in accordance with Section 14.6 of this ordinance. Such a requirement will be included in any deed, lease, purchase and sale agreement, or document transferring or expressing an intent to transfer any interest in real estate or structure, including but not limited to a time-share interest. The condition shall clearly articulate that the municipality may enforce any violation of the construction requirement and that fact shall also be included in the deed or any other document previously described. The construction requirement shall also be clearly stated on any map, plat, or plan to be signed by the Planning Board or local reviewing authority as part of the approval process.

**14.9 Appeals And Variances**

The Board of Appeals of the Town of Buxton may, upon written application of an aggrieved party, hear and decide appeals from determinations of the Code Enforcement Officer in the administration of the provisions of this Ordinance pursuant to Article 6 of the Zoning Ordinance.

The Board of Appeals may grant a variance from the requirements of this Ordinance consistent with state law and the following criteria:

14.9.A Variances shall not be granted within any designated regulatory floodway if any increase in flood levels during the base flood discharge would result.

14.9.B. Variances shall be granted only upon:

14.9.B.1. a showing of good and sufficient cause; and,

14.9.B.2. a determination that should a flood comparable to the base flood occur, the granting of a variance will not result in increased flood heights, additional threats to public safety, public expense, or create nuisances, cause fraud or victimization of the public or conflict with existing local laws or ordinances; and,

14.9.B.3. a showing that the issuance of the variance will not conflict with other state, federal or local laws or ordinances; and,

14.9.B.4. a determination that failure to grant the variance would result in "undue hardship," which in this sub-section means:

14.9.B.4.a. that the land in question cannot yield a reasonable return unless a variance is granted; and,

14.9.B.4.b. that the need for a variance is due to the unique circumstances of the property and not to the general conditions in the neighborhood; and,

14.9.B.4.c that the granting of a variance will not alter the essential character of the locality; and,

14.9.B.4.d that the hardship is not the result of action taken by the applicant or a prior owner.

14.9.Variances shall only be issued upon a determination that the variance is the minimum necessary, considering the flood hazard, to afford relief.

1. Variances may be issued for new construction, substantial improvements, or other development for the conduct of a functionally dependent use provided that:

14.9.D.1. Other criteria of Section 14.9 and Section 14.6.K. are met; and,

14.9.D.2. The structure or other development is protected by methods that minimize flood damages during the base flood and create no additional threats to public safety.

1. Variances may be issued for the repair, reconstruction, rehabilitation, or restoration of Historic Structures upon the determination that:

14.9.E.1. the development meets the criteria of Section 14.9, paragraphs A. through D. above; and,

14.9.E.2. The proposed repair, reconstruction, rehabilitation, or restoration will not preclude the structure’s continued designation as a Historic Structure and the variance is the minimum necessary to preserve the historic character and design of the structure.

1. Any applicant who meets the criteria of Section 14.9, paragraphs A. through E. shall be notified by the Board of Appeals in writing over the signature of the Chairman of the Board of Appeals that:

14.9.F.1. the issuance of a variance to construct a structure below the base flood level will result in greatly increased premium rates for flood insurance up to amounts as high as $25 per $100 of insurance coverage;

14.9.F.2. such construction below the base flood level increases risks to life and property; and,

14.9.F.3. the applicant agrees in writing that the applicant is fully aware of all the risks inherent in the use of land subject to flooding, assumes those risks and agrees to indemnify and defend the municipality against any claims filed against it that are related to the applicant's decision to use land located in a floodplain and that the applicant individually releases the municipality from any claims the applicant may have against the municipality that are related to the use of land located in a floodplain.

14.9.G The Board of Appeals shall submit to the Code Enforcement Officer a report of all variance actions, including justification for the granting of the variance and an authorization for the Code Enforcement Officer to issue a Flood Hazard Development Permit, which includes any conditions to be attached to said permit.

* 1. **Enforcement And Penalties**

1. It shall be the duty of the Code Enforcement Officer to enforce the provisions of this Ordinance pursuant to Title 30-A MRSA § 4452.
2. The penalties contained in Title 30-A MRSA § 4452 shall apply to any violation of this Ordinance.
3. In addition to any other actions, the Code Enforcement Officer, upon determination that a violation exists, shall submit a declaration to the Administrator of the Federal Insurance Administration requesting a denial of flood insurance. The valid declaration shall consist of;
   1. the name of the property owner and address or legal description of the property sufficient to confirm its identity or location;
   2. a clear and unequivocal declaration that the property is in violation of a cited State or local law, regulation, or ordinance;
   3. a clear statement that the public body making the declaration has authority to do so and a citation to that authority;
   4. evidence that the property owner has been provided notice of the violation and the prospective denial of insurance; and,
   5. a clear statement that the declaration is being submitted pursuant to Section 1316 of the National Flood Insurance Act of 1968, as amended.

**14.11 Conflict With Other Ordinances**

This Ordinance shall not in any way impair or remove the necessity of compliance with any other applicable rule, ordinance, regulation, bylaw, permit, or provision of law. Where this Ordinance imposes a greater restriction upon the use of land, buildings, or structures, the provisions of this Ordinance shall control.